[Date Prev][Date Next] [Chronological] [Thread] [Top]

# Numeric Key row inoperable using BS 4.1.1.1

- To: "Bugtrack@Gesn. Com" <bugtrack@dieboldes.com>
- Subject: Numeric Key row inoperable using BS 4.1.1.1
- From: "Larry Dix" <ljdglobal@dieboldes.com>
- Date: Tue, 25 Sep 2001 10:43:02 -0500
- Cc: "Barry Herron" <barry@dieboldes.com>
- Importance: Normal

The numeric key row above the qwerty keys is inoperable when plugging in a keyboard for use as an input device for VIBS. The numeric keypad to the right of the keyboard is operable. This creates a problem when demonstrating ADA capabilities using a big key keyboard. The big key keyboard does not have a numeric keypad and therefore can not enter numeric commands. The big key keyboard was selected to meet ADA requirements in Texas that require all controls and operable mechanisms to be operable with one hand including a closed fist. Larry J. Dix Vice President of Operations Global Election Systems

- Follow-Ups:
  - RE: Numeric Key row inoperable using BS 4.1.1.1
    - From: "Ken Clark" <ken@dieboldes.com>

- Prev by Date: Re: BallotStation 4.1.1/GEMS 1-17-16 upload to wrong database
- Next by Date: RE: Numeric Key row inoperable using BS 4.1.1.1
- Index(es):
  - Chronological
  - Thread