[Date Prev][Date Next] [Chronological] [Thread] [Top]

# Allow accumulated AVTS results to be stored onto and subsequently uploaded from a Smart memory/ microprocessor card into GEMS

- To: "rcr" <rcr@dieboldes.com>
- Subject: Allow accumulated AVTS results to be stored onto and subsequently uploaded from a Smart memory/ microprocessor card into GEMS
- From: "Jeff Hallmark" <jeffh@dieboldes.com>
- Date: Thu, 28 Feb 2002 13:38:12 -0600
- Importance: Normal

We have 4 counties in Maryland:
Dorchester 100 AVTS
Alegheny 330 AVTS
Prince George 2500 AVTS
Montgomery 2800 AVTS
IMPETUS:
Upcoming Maryland elections.
April 2 City of Bowie in Prince George County 40 AVTS 8 pcts using modem for upload
April 26 High/Middle School election in Montgomery County 340 AVTS 54 locations no modem
Sept 10 Primary
November 5 General
Don Vopalensky, who is in Maryland and in direct contact with all the counties, says that as it stands the two small counties, Dorchester and Alegheny, will not use modems for the rest of the year and t he larger two are undecided. This brings us to the question of uploading election results election night in a timely manner, with the strong possibility that at least one of the larger counties as well as the two smaller counties will not use modem.
As always the expectation is an almost immediate release of election results from the time the polls close,but without modem we would have to physically gather all the pcmcia cards from each vote center location, take them to a central or regional site and upload each card via a limited number of AVTS units set up to be accumulators that are networked together. At (2) minutes per card (2500 in Prince George) it will take about 83 hours to complete the upload.Of course this is calculated on using just one AVTS for upload but even using 20 upload machines your looking at 4 hours given no complications and that the 2 minutes per card isn't too low an estimate.
RCR:
Using the Accumulator in AVTS R6, allow a transfer method of storing results onto a "Smart card".
The Smart card that is to be used has been created and ( uniquely encoded) by GEMS or Card Manager as an accumulator card.
Upload into GEMS via networked AVTS or stand alone Smart Card Reader attached to GEMS host.
JUSTIFICATION:
Upload r esults as quickly as possible.
Jeff Hallmark
Diebold Election Systems
jeffh@dieboldes.com
PHN (972) 542 6000 X167
FAX (972) 542 6044

- Follow-Ups:
  - RE: Allow accumulated AVTS results to be stored onto and subsequently uploaded from a Smart memory/ microprocessor card into GEMS
    - From: "Jeff Hintz" <jhglobal@earthlink.net>

- Prev by Date: Allow accumulated AVTS results to be stored onto and subsequently uploaded from a pcmcia card into GEMS
- Next by Date: RE: Allow accumulated AVTS results to be stored onto and subsequently uploaded from a Smart memory/ microprocessor card into GEMS
- Index(es):
  - Chronological
  - Thread