[Date Prev][Date Next] [Chronological] [Thread] [Top]

# RE: R6 modem testing successful

- To: <support@gesn.com>
- Subject: RE: R6 modem testing successful
- From: "Ken Clark" <ken@gesn.com>
- Date: Wed, 16 Jan 2002 17:09:41 -0800
- Importance: Normal
- In-reply-to: <026101c19ef1$8c30cd40$1ddbfc9e@default>

From: owner-support@gesn.com [mailto:owner-support@gesn.com]On Behalf Of Steve Knecht Sent: Wednesday, January 16, 2002 4:55 PM 3. Since the phone number isn't on a PCMCIA card (I understand the Accumulation process doesn't write totals to any of the PCMCIA cards (I think this will have to change) then either we put phone numbers on all PCMCIA cards in the precinct or the pollworker must have to type in the phone number? How does that work? The phone number is on the PC card (or it should be anyway). You enter the phone number in the vote center dialog in GEMS before memory cards are created. Ken

- Follow-Ups:
  - Re: R6 modem testing successful
    - From: "Tari Runyan" <trglobal@earthlink.net>
  - Re: R6 modem testing successful
    - From: "Greg Forsythe" <gfglobal@earthlink.net>

- References:
  - Re: R6 modem testing successful
    - From: "Steve Knecht" <skglobal@earthlink.net>

- Prev by Date: RE: Nearterm AVTS 4.x roadmap
- Next by Date: Re: R6 modem testing successful
- Index(es):
  - Chronological
  - Thread