[Date Prev][Date Next] [Chronological] [Thread] [Top]

# RE: Central Count Error Messages

- To: <bugtrack@dieboldes.com>
- Subject: RE: Central Count Error Messages
- From: "Ken Clark" <ken@dieboldes.com>
- Date: Thu, 2 Mar 2000 14:13:04 -0600
- Importance: Normal
- In-reply-to: <000e01bf8483$2bdd7860$20f6f7d1@stevek.dieboldes.com>

What firmware? 2.00g was supposed to address this specifically: Adjusted the timing mark signal filtering to reduce the number of non-processed ballots. Ken We have started counting absentee ballots in Marin. We are getting a significant number of the following error messages. NO ENDER MARK - the ballot will usually be taken on the next try NO BACK LEFT TIMING MARK (0 or 52) - these also run on next try or so. I've looked at the ballots and find no discernable reason for them to be stopping or giving this message, as they have all appropriate timing marks. I don't expect there's anything to be done, but it could be looked at prior to next election.

- References:
  - Central Count Error Messages
    - From: "Steve Knecht" <skglobal@earthlink.net>

- Prev by Date: Central Count Error Messages
- Next by Date: Re: Central Count Error Messages
- Index(es):
  - Chronological
  - Thread